Batch CAD Cart (0) ▾

- Cart is empty

1. Click Here for Batch CAD Downloads

Online literature contains the most current information available.
Request Information
The PEMSERTER® Series 4® insertion machine is totally pneumatic providing short cycle time for increased productivity and 53.4 kN / 6 tons of force and a 45.7 cm / 18” throat depth which provides clearance for a variety of chassis configurations. It is designed to install self-clinching fasteners in size M2 / #0 thru M10 / 3/8” in steel, and sizes up to M12 / 1/2” in aluminum panels or circuit boards.
Features and Benefits

- Insertion force adjustable from 1.8 to 53.4 kN / 400 to 12,000 lbs..
- Pneumatic power for speed, consistency, and simple operation. Requires shop air only.
- Integral point-of-operation safety.
- Adjustable positive ram stop.
- Large parts tray with dividers.
- Rapid tooling changeover, perfect for short production runs.
- Laser pointer, stroke counter, and lockable cabinet for tools and accessories storage.
- One-year parts warranty and two-year limited warranty on pneumatic components.

Unit of Measure

- Specifications

## Ram Force | N/A 4.5 to 53.4 kN1000 to 12000 lb
## Control System | N/A Pneumatic Logic
## Pressure System Type | N/A Pneumatic / Lever
## Air Requirements | N/A 6 to 7 bar / 90 to 100 psi 12 mm / 1/2 in dia. minimum line flow
## Throat Depth | N/A 45.70 cm18 in
## Height | N/A 167.60 cm66.00 in
## Width | N/A 43.20 cm17.00 in
## Weight | N/A 259.00 kg570.0 lb
## Weight with Cabinet | N/A 372.00 kg819.00 lb
## Cabinet Dimensions L x W x H | N/A 74.00 x 66.00 x 76.00 cm29.00 x 26.00 x 30.00 in

Required Fields *

Email * |
First Name * |
Last Name * |
Company * |
Country * |
Zip/Postal Code * |
Phone Number * |
User Information | How is your information being used? View Privacy Policy

Required Fields *

Email * |
First Name * |
Last Name * |
Project Name |
Project Location |
Title |
Company * |
Country * |
Country * |
City * |
Zip/Postal Code * |
Phone Number * |
Job Title |